Part 1.	Automated Lighting
1.01	White-light, Light Emitting Diode FRAMING Moving head fixture 
A.	General
1.	The fixture shall be a high-intensity white-light fixture with Cyan, Magenta, Yellow and CTO subtractive color mixing. The fixture shall be a SolaSpot 2000 by High End Systems or approved equivalent. 
2.	All LED moving light fixtures shall be provided by a single manufacturer to ensure compatibility.
3.	The fixture shall be UL 1573 listed for stage and studio use and comply with EN60598-2-17 standard per CE certification
4.	The fixture shall comply with the USITT DMX-512A standard, 
B.	Physical or Mechanical
1.	The fixtures structural framing shall be constructed of rugged, 1/8” aluminum, free of burrs and pits.
2.	Outer covers of head and yoke shall be constructed of ABS plastic with fine textured black surface and fastened to the head frame with quarter turn fasteners.
3.	The fixture dimensions shall be 
a.	838 mm (33”) from base of the enclosure, to the tip of the lens baffling.  
b.	475 mm (18.7”) across the exterior dimensions of the yolk
c.	The Electronics enclosure shall be 320 mm (12.6”) Wide 
d.	Head length 587 mm (23.1”) 
e.	Fixture shall weigh 42 kg (92 lbs.)
4.	The fixture shall be able to be either truss mounted or set upright on a stable surface. Fixture shall be suitably designed for operation over or under mounted on a truss perpendicular to the ground as well as outrigged parallel to the ground.
5.	The following shall be provided:
a.	The fixture must include two gobo wheels with six (6) interchangeable rotating gobos each.  
1)	Gobo Size shal be 30mm outside diameter and 25mm image area.  
2)	Rotating gobo systems must be able to index to any point on the 360 positioning of the gobo.  
3)	Rotating gobos must be interchangeable with glass and metal gobo patterns without permanent or semi-permanent modification to the wheels or cartridges.
b.	CMY (Cyan Magenta Yellow) and CTO (Color Temperature – Orange) subtractive color mixing system plus seven (7) interchangeable colors including red, blue, green, yellow, orange, purple, and dark blue.
c.	Lens defogging system for preventing atmospheric haze or environmental fog materials from building up and limiting output during operation.  Fixtures that do not deploy lens defogging systems shall not be deemed acceptable.
d.	Fixture shall have 540 degrees of pan and 265 degrees of tilt.  Pan and tilt must be controlled with 16bit control and utilize encoder sensors to guarantee correct step position.
1)	Fixture shall have a pan speed of 3.66s for 360 degree movement
2)	Fixture shall have a tilt speed of 2.59s for 252 degree of movement.
3)	Pan and tilt locks that stop at 0, 45, and 90 degrees for service and handling. Pan and tilt locks are not intended to be engaged during transport in pre-rigged truss.
e.	A 16 leaf iris which reduces the projection area by 92%.
f.	Frost system which softens the edges of the projection on a surface that applies evenly across the beam and allows for variation in insertion time. 
g.	Automated 7-47 zooming lens system.
h.	Two animation wheels that allow for continuous and uninterrupted motion in two directions and can be moved in/out of the beam.
i.	Two Prisms that include:
1)	Triangular three facet prism 
2)	Four facet linear prism
3)	Both prisms must be index able, and continuously rotatable in both clockwise and counterclockwise directions. 
6.	Power supply, cooling and electronics shall be integral to each unit.
7.	The unit shall ship with:
a.	5’ Neutrik True1 PowerCon™ to wire ferrule as standard
b.	Two (2) brackets that facilitate attaching standard brackets to the fixture base via ¼ turn thumb screws.
c.	One (1) safety cable.
C.	Optical
1.	The light emitting diode engine shall produce 6500K white light within +/-500K
2.	The light engine shall be designed to create a color rendering at greater than 70 CRI 
3.	The fixture shall produce 25,000 field lumens with all LED’s at full
4.	The unit shall provide, but not be limited to:
a.	Low gate and beam temperature
b.	Sharp Imaging on all gobo and Iris planes
5.	The unit shall provide, but not be limited to:
a.	7 through 47 degree field angles
b.	Adjustable hard and soft beam edges. Systems that fail to soften beam edges while also achieving crisp single edge, when desired, without blue or brown halation shall be deemed unacceptable.
D.	Environmental and Agency Compliance 
1.	The fixture shall be ETL and cETL LISTED and/or CE rated, and shall be so labeled when delivered to the job site.
2.	The fixture shall be ETL LISTED to the UL1573 standard for stage and studio use 
3.	The fixture shall be rated for IP-20 dry location use.
4.	When the fixture is stationary, and at full intensity, the fixture may not produce noise in excess of 38 dBA.  A fixture that produces noise in excess of 38 dBA when stationary and at full intensity shall be deemed unacceptable. 
a.	At no time may the fixture produce noise in excess of 50.8 dBA.
1)	All dBA numbers above are tested in a test chamber with background noise level of 32 dBA.
E.	Thermal 
1.	Fixture shall be equipped with a heat pipe radiant cooling system.
2.	The fixture shall utilize advanced thermal management systems to maintain LED life to an average of 70% intensity after 50,000 hours of use 
a.	Fan speed will be capable of automatically adjusting based on thermal management needs.
1)	Fixture will provide three fan speed modes that are selectable via DMX.
b.	Thermal management shall include temperature sensors within the housing to include:
1)	LED array circuit board temperature
c.	Fixture user shall permit monitoring of temperature sensors via a legible LCD multi-line backlit display
d.	Fixtures that do not provide active thermal monitoring, fan speed controls, and current management of LED circuits shall not be acceptable.
3.	The fixture shall operate in an ambient temperature range of 0°C (32°F) minimum, to 45° C (113°F) maximum ambient temperature. During times of storage, the fixture shall be stored in temperatures range of -20C (0°F) to 60C (140°F)
4.	The fixture shall maintain .5m (1.64 feet) distance from any flammable object
5.	The fixture shall maintain a minimum of 1.5m (4.9 feet) to any lighted object.
F.	Electrical
1.	The fixture shall be equipped with a 100V to 240V 50/60Hz auto-sensing internal power supply 
a.	Fixture shall draw a maximum of 10 amps at 100V and 4 amps at 240 V.
2.	The fixture shall support power in and thru operation 
a.	Power in shall be via Neutrik® PowerCon™ True1 input connector
b.	Power thru shall be via Neutrik® PowerCon™ True1 output connector
3.	The fixture requires power from a non-dimmer source. 
4.	Power supply outputs shall have self-resetting current-limiting protection
5.	Power supply shall have power factor correction greater than 0.92 from 90 VAC to 265 VAC.
G.	LED Emitters
1.	All LEDs used in the fixture shall be high brightness and proven quality from established and reputable LED manufacturers. 
a.	Appotronics are the sole manufacture of approved emitter engines.
2.	Manufacturer of LED emitters shall utilize an advanced production LED binning process to maintain color consistency.
3.	All LED fixtures (100% of each lot) shall undergo a minimum 12-hour burn-in test during manufacturing.
4.	LED system shall comply with all relevant patents
5.	Fixtures shall have PWM frequency up to 16,000hz to avoid flicker on camera
H.	Calibration
1.	Fixture shall be calibrated at factory for achieve consistent color and intensity output between fixtures built at different times and/or from different LED lots or bins
a.	All arrays, including replacement arrays shall be calibrated to the same standard to insure consistency.
I.	Color
1.	The fixture shall be available in specialized LED arrays as outlined below:
a.	Ultra-Brite 6500k white light engine
1)	White LED Engine calibrated and binned to achieve 6500k (+/- 500k).
a)	Measured brightness of Ultra-Brite 6500k engine shall be greater than 25,000 Lumens when tested in an integrating sphere.
2.	Fixture must have a subtractive color mixing system utilizing eight (8) dichroic color flags, controlled in pairs, to linearly subtract the following colors out of fixtures light output.
a.	Cyan
b.	Magenta
c.	Yellow
d.	Color Temperature – Orange
3.	Fixture must have semi trapezoidal dichroic glass color segments on a single wheel that transmit the following colors.  Dichroics must be replaceable without removal or application of adhesive.
a.	Red
b.	Green
c.	Blue
d.	Yellow
e.	Orange
f.	Purple
g.	Dark Blue
J.	Dimming
1.	The LED system shall use 16-bit DMX control techniques for high-resolution dimming.
2.	Dimming curves shall be optimized for smooth dimming over longer timed fades. 
3.	The LED system shall be digitally driven using high-speed pulse width modulation (PWM)
K.	Control and User interface
1.	Ethernet compatible with support for ANSI1.31 Streaming ACN and ArtNet protocols
2.	Fixture must provide an internal Ethernet switch that supports both active and passive data pass-through.
3.	Fixtures shall be capable of supporting protocol conversion from Ethernet to DMX output.
4.	The fixture shall be USITT DMX 512A-compatible via In and Thru 5-pin XLR connectors 
5.	The fixture shall be compatible with the ANSI RDM E1.20 standard
a.	All fixture functions shall accessible via RDM protocol for modification from suitably equipped control console
b.	Temperature sensors within the luminaire shall be viewable in real time via RDM.
c.	Fixtures not offering RDM compatibility, feature set access or temperature monitoring via RDM shall not be compatible
6.	The fixture shall be equipped with multi-line color LCD display for easy-to-read status reports and configuration changes.
a.	Display must have a feature to battery power the menu structure when the fixture is unplugged to allow fixture settings to be adjusted, including DMX.
7.	The fixture shall be equipped with a six-button user-interface
8.	The fixture may offer no more than a single DMX control profile.  
a.	Fixture DMX Control Profile will have 43 channel control.