Part 1.	Automated Lighting
1.01	White-light, Light Emitting Diode FRAMING Moving head fixture 
A.	General
1.	The fixture shall be a high-intensity white-light fixture with Cyan, Magenta, Yellow and CTO subtractive color mixing as well as framing shutters. The fixture shall be a SolaWash 2000 by High End Systems or approved equivalent. 
2.	All LED moving light fixtures shall be provided by a single manufacturer to ensure compatibility.
3.	The fixture shall be UL 1573 listed for stage and studio use and comply with EN60598-2-17 standard per CE certification
4.	The fixture shall comply with the USITT DMX-512A standard
B.	Physical or Mechanical
1.	The fixtures structural framing shall be constructed of rugged, 1/8” aluminum, free of burrs and pits and finished with a matte black powder coating.
2.	Outer covers of head and yoke shall be constructed of ABS plastic with fine textured black surface and fastened to the head frame with quarter turn fasteners.
3.	The fixture dimensions shall be 
a.	886 mm (34.9”) from base of the enclosure, to the tip of the lens baffling 
b.	475 mm (18.7”) across the exterior dimensions of the yolk
c.	The Electronics enclosure shall be 304mm (12”) Wide 
d.	Head length 638 mm (25.1”) 
e.	Fixtures shall weigh 42kG (92lbs)
4.	The fixture shall be able to be either truss mounted or set upright on a stable surface. Fixture shall be suitably designed for operation over or under mounted on a truss perpendicular to the ground as well as outrigged parallel to the ground.
5.	The following shall be provided:
a.	Shutter assembly shall be a four plane system capable of rotating +/- 30 and fully crossing the beam on each individual shutter blade.  Additionally the entire Shutter assembly must rotate +/- 45 . 
b.	CMY (Cyan Magenta Yellow) and CTO (Color Temperature – Orange) subtractive color mixing system six (6) interchangeable colors including red, blue, green, orange, purple, and dark blue.
c.	Includes a secondary fixed color wheel with sig (6) non-interchangeable colors including magenta, pink, minus green, two levels of CTB, and amber.
d.	Lens defogging system for preventing atmospheric haze or environmental fog materials from building up and limiting output during operation.  Fixtures that do not deploy lens defogging systems shall not be deemed acceptable.
e.	Fixture shall have 540 degrees of pan and 265 degrees of tilt.  Pan and tilt must be controlled with 16bit control and utilize encoder sensors to guarantee correct step position.
1)	Fixture shall have a pan speed of 3.66s for 360 degree movement
2)	Fixture shall have a tilt speed of 2.59s for 252 degree of movement.
3)	Pan and tilt locks that stop at 0, 45, and 90 degrees for service and handling. Pan and tilt locks are not intended to be engaged during transport in pre-rigged truss.
f.	A 16 leaf iris which reduces the projection area by 97%.
g.	Two dual flag frost systems that can be used simultaneously, or independently, to soften the beam and projection edges.
h.	Automated 5 - 50 zooming lens system.
6.	The yolk arms must have collapsible, spring loaded, handles for fixture handling and manipulation.
7.	Power supply, cooling and electronics shall be integral to each unit.
8.	The unit shall ship with:
a.	5’ Neutrik PowerCon™ to wire ferrule as standard
b.	Two (2) brackets that facilitate attaching standard brackets to the fixture base via ¼ turn thumb screws.
C.	Optical
1.	The light emitting diode engine shall produce 7400K white light within +/-500K
2.	The light engine shall be produce a color rendering index at greater than 75 CRI 
3.	The fixture shall produce up to 26,000 field lumens with all LED’s at full
4.	The unit shall provide, but not be limited to:
a.	Low gate and beam temperature
b.	Soft edge imaging on a four-plane, four shutter design.  Systems that do not have four independently controlled shutters on independent planes of travel shall be deemed unacceptable.
5.	The unit shall provide, but not be limited to:
a.	5 through 50 degree field angles
D.	Environmental and Agency Compliance 
1.	The fixture shall be ETL and cETL LISTED and/or CE rated, and shall be so labeled when delivered to the job site.
2.	The fixture shall be ETL LISTED to the UL1573 standard for stage and studio use 
3.	The fixture shall be rated for IP-20 dry location use.
4.	When the fixture is stationary, and at full intensity, the fixture may not produce noise in excess of 38 dBA. 
E.	Thermal 
1.	Fixture shall be equipped with a passive heat pipe radiant cooling System.
2.	The fixture shall utilize advanced thermal management systems to maintain LED life to an average of 70% intensity after 50,000 hours of use 
a.	Fan speed will be capable of automatically adjusting based on thermal management needs.
1)	Fixture will provide three fan speed modes that are selectable via DMX.
b.	Thermal management shall include multiple temperature sensors within the housing to include:
1)	LED array circuit board temperatures
c.	Fixtures that do not provide active thermal monitoring and current management of LED circuits shall not be acceptable.
3.	The fixture shall operate in an ambient temperature range of 0°C (32°F) minimum, to 45° C (113°F) maximum ambient temperature. During times of storage, the fixture shall be stored in temperatures range of -20C (0°F) to 60C (140°F)
4.	The fixture shall maintain .5m (1.64 feet) distance from any flammable object
5.	The fixture shall maintain a minimum of 1.5m (4.9 feet) to any lighted object.
F.	Electrical
1.	The fixture shall be equipped with a 100V to 240V 50/60Hz auto-sensing internal power supply 
a.	Fixture shall draw a maximum of 8.6 amps at 100V and 3.5 amps at 240 V.
2.	The fixture shall support power in and thru operation 
a.	Power in shall be via Neutrik® PowerCon™ input connector
3.	The fixture requires power from a non-dimmer source 
4.	Power supply outputs shall have self-resetting current-limiting protection
G.	LED Emitters
1.	All LEDs used in the fixture shall be high brightness and proven quality from established and reputable LED manufacturers. 
a.	Appotronics are the sole manufacture of approved emitter engines.
2.	Manufacturer of LED emitters shall utilize an advanced production LED binning process to maintain color consistency.
3.	All LED fixtures (100% of each lot) shall undergo a minimum 12-hour burn-in test during manufacturing.
4.	LED system shall comply with all relevant patents
5.	Fixtures shall have PWM frequency up to 16,000hz to avoid flicker on camera
H.	Color
1.	The fixture shall be available in specialized LED arrays as outlined below:
a.	Ultra-Brite 7400k white light engine
1)	White LED Engine calibrated and binned to achieve 7400k (+/- 500k) with a minimum of 75 CRI.
a)	Measured brightness of Ultra-Brite Engine shall be greater than 26,000 lumens when tested in an integrating sphere.
b.	High CRI 6500k white light engine
1)	White LED Engine calibrated and binned to achieve 6500k (+/- 500k) with a minimum of 90 CRI.
a)	Measured brightness of High CRI 6500k engine shall be greater than 20,000 Lumens when tested in an integrating sphere.
c.	High CRI 3200k white light engine
1)	White LED Engine calibrated and binned to achieve 3200k (+/- 250k)
2.	Fixture must have a subtractive color mixing system utilizing eight (8) dichroic color flags, controlled in pairs, to linearly subtract the following colors out of fixtures light output.
a.	Cyan
b.	Magenta
c.	Yellow
d.	Color Temperature – Orange
3.	Fixture must have semi trapezoidal dichroic glass color segments on a single wheel that transmit the following colors.
a.	Red
b.	Green
c.	Blue
d.	Orange
e.	Purple
f.	Dark Blue
4.	Fixture must have semi trapezoidal dichroic glass color segments on a second single wheel that transmit the following colors.
a.	Magenta
b.	Pink
c.	Minus Green
d.	CTB – 1
e.	CTB – 2
f.	Amber
5.	Fixture must have a TM-30 filter available as an optional accessory.  This filter will use a subtractive dichroic to increase the fixtures CRI values to greater than 85 CRI at the expense of light output. 
I.	Dimming
1.	The LED system shall use 16-bit DMX control techniques for high-resolution dimming.
2.	Dimming curves shall be optimized for smooth dimming over longer timed fades. 
3.	The LED system shall be digitally driven using high-speed pulse width modulation (PWM)
4.	LED control shall be compatible with broadcast equipment in the following ways:
a.	PWM control of LED levels shall be imperceptible to video cameras and related equipment
J.	Control and User interface
1.	The fixture shall be USITT DMX 512A-compatible via In and Thru 5-pin XLR connectors and In and Thru 3-pin XLR connectors.
2.	The fixture shall be compatible with the ANSI RDM E1.20 standard
a.	All fixture functions shall accessible via RDM protocol for modification from suitably equipped control console
b.	Fixtures not offering RDM compatibility, feature set access or temperature monitoring via RDM shall not be compatible
3.	The fixture shall be equipped with multi-line color LCD display for easy-to-read status reports and configuration changes.
a.	Display must have a feature to battery power the menu structure when the fixture is unplugged to allow fixture settings to be adjusted, including DMX.
4.	The fixture shall be equipped with a six-button user-interface
5.	The fixture may offer no more than a single DMX control profile.  
a.	Fixture DMX Control Profile will have 36 channel control.