Hoglet 4 Programming Wing
A. General:
1.	The lighting control programming wing shall be a Hoglet 4. The console shall be available from High End Systems, Inc., 2105 Gracy Farms Lane, Austin, TX 78758, USA.
2.	The lighting control system shall be designed specifically for the control of stage, studio, touring, entertainment and architainment lighting systems.
3.	A company having over 20 years of experience in the control of entertainment lighting shall manufacture the lighting control system.
4.	The equipment shall be ETL listed.
5.	Systems that do not provide the features listed below shall not be acceptable.
B. Hardware:
1.	The programming wing shall be constructed of a rugged aluminum chassis with powder coated panels and faceplates. An arm rest shall be provided.
2.	An external 12VDC power supply shall be provided.
3.	Controls shall consist of keypad, four (4) rotary encoders and twelve (12) User Keys. There shall be ten (10) user programmable, Alps faders with associated illuminated enable buttons on the playback portion of the console. 
4.	One (1) desk light is provided, using dimmable white LEDs for illumination. 
5.	In conjunction with a connected Hog 4 PC computer, the programming wing shall be capable of outputting four (4) DMX universes via a built-in Super Widget with 5-pin XLR connectors.
6.	MIDI and SMPTE Timecode functionality may be added through use of external widgets.
7.	The following interfaces shall be provided
a.	Two (2) Universal Serial Bus ports
b.	One USB B input connector
c.	Four (4) 5-pin XLR DMX outputs
8.	The console shall be 603mm/23.8” wide by 314mm/12.4” deep by 67mm/2.6” high, weighing 3.9kg/8.7lb.
9.	The user shall make operating software upgrades via USB. No changing of internal components shall be required. 
10.	The control console shall be supplied with
a.	12VDC Power Supply Unit
b.	Dust cover
c.	Desk light (white)
d.	USB cable
e.	USB flash drive (show storage)

C. Programming and playback:

1.	When connected to a Hog 4PC computer or Rack Hog 4 device, the programming wing’s capacities shall be: 2048 local output channels/parameters, an unlimited number of simultaneous crossfades, and up to 65,536 cues, cue lists, chases, scenes, palettes, groups, and pages. There shall be no specific limit on the number of DMX universes supported when DMX processor units are connected.
2.	The controller shall provide unlimited simultaneous playback of independent cue lists, chases, or scenes on up to ten (10) Playback masters on the programming wing. Additional Playback masters may be added with expansion wing units and virtual masters. Masters shall also be able to provide inhibitive intensity control of some or all fixtures.
3.	Cue lists, scenes, and inhibitives shall be dynamically assigned to Masters and grouped together on a Page. Changing Pages shall load a new set of cue lists, scenes and inhibitives to the Masters.
4.	The controller shall possess advanced Page features including: instant changes, crossfading between pages, flexible sizes, automatic holdover and remain in background.
5.	Custom settings shall be provided for Go and Flash buttons, Cues, Cuelists, and submasters including but not limited to activation, precedence (HTP or LTP), resetting, inhibitive.
6.	There shall be a main set of playback controls providing Go, Halt/Back, Step Forward, Step Back, Go To, Release and Assert buttons.
7.	User Keys shall be represented as an element of the graphical user interface of the Hog 4 software, contained on a connected PC or Rack Hog 4 device.

D. Provide the following
Qty 	Part number 	Description
- 	61020004 	Hog 4 console in road case 
-	61020005	Full Boar 4 console in road case
-	61020006	Road Hog 4 console
-	61020011	HedgeHog 4 console
-	61020014	HedgeHog 4X console
- 	62040004 	DMX Processor 8000 (8192 channels, rack mount)
- 	74040007 	USB DMX Widget 
- 	74040008 	USB Super Widget 
- 	62040005 	USB DMX Super Duper Widget
- 	74040009 	USB MIDI/LTC Widget 
-	61040060 	Playback Wing 4
- 	61040062 	Master Wing 4
-	61040065	MiniWing 4
-	61040064	Hoglet 4 programming wing
- 	90903067 	Hog USB show storage flash drive (black)
- 	90903068 	Hog USB system restore flash drive (red)
- 	61040109 	Super Widget expansion kit
-	74040010	MIDI/LTC expansion kit
- 	61070012 	Playback/Master Wing 4 road case
-	61070011	Road Hog 4 road case
-	99330191	HedgeHog 4 soft carry bag
-	61070015	HedgeHog 4 Gator hard case
-	61070014	HedgeHog 4 custom road case
-	61070016	Hoglet 4 road case
-	61070017	MiniWing 4 road case
- 	61100004 	Hog white/blue desk light (extra)